0 Bottom column total dimensions to be given in plan (0:No, 1:Yes)
0 Bottom column break-up dimensions to be given in plan (0:No, 1:Yes)
0 Top column total dimensions to be given in plan (0:No, 1:Yes)
0 Top column break-up dimensions to be given in plan (0:No, 1:Yes)
1 DecaPlot sheet border
0 Beam nos. in sectional elevation (0:No, 1:Yes)
0 Column nos. in sectional elevation (0:No, 1:Yes)
0 Cross beam nos. in sectional elevation (0:No, 1:Yes)
0 Cross slab nos. in sectional elevation (0:No, 1:Yes)
2 Stirrups as per 13920 upto L/4
1 Split beam no. & beam size in plan (0:No, 1:Yes, 2: Beam mark only)
0 First span left X-section of beams (0:No, 1:Yes)
0 First span middle X-section of beams (0:No, 1:Yes)
0 Intermediate & End span left X-section of beams (0:No, 1:Yes)
0 Intermediate & End span middle X-section of beams (0:No, 1:Yes)
0 End span right X-section of beams (0:No, 1:Yes)
0 Bar marks & BBS for slab r/f (0:No, 1:Yes)
1 A4 Sheet size for BBS (0:No, 1:Yes)
25 Mix for Laps
4 (Beam marking style 0:Staad Nos, 1:BX1,BY1 First to Last , 2:B1,B2 Every Span, 3:B1, B2 Every Span with Beam Size in Every Span in Elevation, 4:B1,B2 First to Last )
0 Beam schedule (0:No, 1:Yes, 2: Yes with bar shapes, 3: Compact beam)
0 Support r/f curtailment as per max. of ajacent spans (0:No, 1:Yes)
0 Slab Mark (0:No Slab Mark, 1:S1, S2 etc., 2: SLD Slab Mark)
0 Default Title Block
0 All Long Bars, No Short Bars
0 Stirrups in beam elevation
1 Layout required
0 Donot draw stirrups in beam elevation
True
False
False
False
0.75
0.75
300
500
2000
500
0 Ast in Sq.cm (0: Sq.cm, 1: Sq.mm)
-  Prefix
0 Red Cross on Failing Beams (0:No, 1:Yes)
1
1
1
1 Beam Layout Required
1 Beam Elevations Required
