0 STIRRUP LINE IN BEAM ELEVATION IPLOTSTPLINE = 0 NO STP LINE, = 1 STP LINE DRAWN (DEFAULT 0)
2 ITYPESTP

ITYPESTP = 0: 1 LINE TEXT - DIA OUT SIDE IF STIRRUP LEGS & DIA SAME FOR ALL SPANS,
                & = 1 AUTO, 2 LINE TEXT AUTO IF STIRRUP LEGS OR DIA VARY IN ANY SPAN
         = 1: 2 LINE TEXT ALWAYS
         = 2: STRIRRUP DIA. AND SPACING IN 1 LINE OR 2 LINES
              DEPENDING ON AVAILABLE SPACE 19 MM FOR 8 DIA & 21 MM FOR OTHER DIA
(DEFAULT 0)

SPACE REQD. FOR 1 LINE TEXT:
19 MM FOR 8 DIA.
21 MM FOR > 8 DIA
